

AFGHANISTAN CRICKET BOARD

REQUEST FOR QUOTATIONS (RFQ) FOR

PROCUREMENT OF

***Installation of Drip irrigation system for Kunduz, Zabul & Helmand cricket grounds***

*02, Dec, 2024*

**Instructions to Users**

This instruction notes have been prepared to assist a Procuring Entity/user in the preparation of the Standard Request for Quotations (SRFQ) for procurement of Goods and non-consultancy services. The Procuring Entity/user should also refer to the procurement manual date 2022 of RFQ.

The use of SRFQ applies when a Procuring Entity/user (the Purchaser) wishes to select a Supplier for the procurement of Goods and non-consultancy services as per procurement manual.

The confirmation of the Award should be in the form of a Contract, prepared by the Procuring Entity, attached to which will be the Conditions of Purchase. The contract will be signed by both the Procuring Entity and the Supplier and will be treated as contract. Signing of a separate contract is not required.

Prior to the detailed evaluation of Quotations, the Contract shall determine whether each Quotation:

1. meets the eligibility criteria;
2. has been properly signed;
3. Is substantially responsive to the requirements of the Request for Quotations Documents

Evaluation of Quotations

A substantially responsive Quotation is one which conforms to all the terms, conditions, and specifications of the Request for Quotations Documents.

To evaluate a Quotation, the Purchaser shall only use all the factors, methodologies and criteria defined hereinafter, no other criteria or methodology shall be permitted:

1. evaluation will be done for Items or Lots;
2. price adjustment for correction of arithmetic errors;
3. price adjustment due to discounts offered;
4. Adjustments due to the application of a margin of preference, if applicable.

If a Quotation is not substantially responsive, it shall be rejected by the Purchaser, and may not subsequently be made responsive by correction or withdrawal of the nonconforming deviation or reservation.

No negotiation shall be held with the lowest or any other Bidder.

A bidder shall not be required, as a condition for award, to undertake responsibilities not stipulated in the Request for Quotations Documents, to have to change its price or otherwise modify its Quotation.

**Request for Quotation for**

**Installation of Drip irrigation system for Kunduz, Zabul & Helmand cricket grounds**

**Reference:** *ACB/ICC/PRO/GO/2024/F&T /AFG/RFQ-39*

Issue Date: Dec,02, 2024

Closing Date: Dec,08,2024

Name of the Supplier: Address of the Supplier: Contact No \_ Email Add:

1. The Afghanistan Cricket Board has a budget allocation for the purchase of Goods; and is applying some of that allocation for the preparing and installation of **drip irrigation system** and other related goods for which this Request for Quotation is issued.
2. Payments made against any Contract arising from this Request for Quotation will only be made in AFN. The Unit Rate(s) offered by the Supplier, if accepted, shall remain fixed for the duration of the contract.

Your sealed quotation must be submitted to ACB main office of the undersigned **ON *Dec,08, 2024* at 10:00 AM** Kabul time. Any quotation received later than the scheduled time will be rejected and returned unopened. The sealed envelope containing the quotation must be clearly marked Providing **installation drip irrigation system** for Kunduz, Zabul and Helmand cricket grounds and do not open before ***Dec,08, 2024 10:00 AM****.*

1. All quotations must be valid for a period of thirty (30) days from the closing date of the Request for Quotations.
2. The quotation shall be completed and all pages shall be signed or stamp by an authorized representative of the Supplier.
3. In the case of any arithmetical discrepancy between the Unit Rate and the Total Amount quoted, then the Unit Rate shall prevail both for the evaluation of quotations and for the subsequent contract.
4. Depending on the final requirement, the quantities shown may increase or decrease by fifteen percent (15%) and this shall be reflected in the contract.
5. There will be no public opening of quotations; the Purchaser is not bound to accept the lowest quotation and reserves the right to accept or reject any or all the quotations without assigning any reason whatsoever.
6. Supplier with valid business license taxable at rate of 2% and supplier without valid business license at rate of 7%.

**Schedule of Items and Priced Quotation including delivery to Kunduz, Zabul & Helmand cricket grounds**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **NO** | **Description** | **Unit** | **Quantity** | **Unit Cost** | **Total Cost** |
| **Zabul Cricket ground Drip irrigation System BOQ** | | | | | |
| 1 | **Turbulent Flowing On-line Dripper, 4L/h, Black Color (made in China or Turkey)** | **Each** | **2,000.00** |  |  |
| 2 | **Offtake for PVC Pipe, Dn,16, With T type Grommet (made in China or Turkey)** | **Each** | **100.00** |  |  |
| 3 | **LLDPE Lateral pipe, outside Dia 16mm, 1.2mm thickness, 4.0bar, Laser print Φ16\*1.2 500m 1m/laser, One Bule Line on pipe** | **Meter** | **1,500.00** |  |  |
| 4 | **HDPE Pipe 1.5" (50mm) SDR 17, PN 10, PE 100 quality (50 years warranty)** | **Meter** | **500.00** |  |  |
| 5 | **HDPE Pipe 1.25" (40mm) SDR 17, PN 10, PE 100 quality (50 years warranty)** | **Meter** | **250.00** |  |  |
| 6 | **Disc Filter filter surface 1200qcm, max pressure 10 bar, max flow 30 (m3/h), 120Mesh, 2"BSP Male Thread, (made in China or Turkey)** | **Each** | **1.00** |  |  |
| 7 | **End Line, Dn16, (made in China or Turkey)** | **Each** | **100.00** |  |  |
| 8 | **Safety Ring, Dn16, (made in China or Turkey)** | **Each** | **200.00** |  |  |
| 9 | **Straight Connector, Dn16, (made in China or Turkey)** | **Each** | **50.00** |  |  |
| 10 | **Stainless Steel Pressure Gauge (L), 3" display, (made in China or Turkey)** | **Each** | **2.00** |  |  |
| 11 | **Fittings set** | **lump-sum** | **1.00** |  |  |
| 12 | **5 HP submersible water pump, capacity 10m3/h (JD, Dongyin, Vackson) along with the required 100m power cable** | **Each** | **1.00** |  |  |
| 13 | **Delivery to Zabul Cricket Ground** | **lump-sum** | **1.00** |  |  |
| 14 | **Excavation of 1200m (30cm deep x 30cm wide) for burying the main pipe** | **Each** | **750.00** |  |  |
| 15 | **Survey, design and Installation** | **lump-sum** | **1.00** |  |  |
| **Sub Total/AFN** | | | | |  |
|  | | | | | |
| **NO** | **Description** | **Unit** | **Quantity** | **Unit Cost** | **Total Cost** |
| **Helmand Cricket ground Drip irrigation System BOQ** | | | | | |
| 1 | **Turbulent Flowing On-line Dripper, 4L/h, Black Color (made in China or Turkey)** | **Each** | **2,000.00** |  |  |
| 2 | **Offtake for PVC Pipe, Dn,16, With T type Grommet (made in China or Turkey)** | **Each** | **100.00** |  |  |
| 3 | **LLDPE Lateral pipe, outside Dia 16mm, 1.2mm thickness, 4.0bar, Laser print Φ16\*1.2 500m 1m/laser, One Bule Line on pipe** | **Meter** | **1,500.00** |  |  |
| 4 | **HDPE Pipe 1.5" (50mm) SDR 17, PN 10, PE 100 quality (50 years warranty)** | **Meter** | **500.00** |  |  |
| 5 | **HDPE Pipe 1.25" (40mm) SDR 17, PN 10, PE 100 quality (50 years warranty)** | **Meter** | **250.00** |  |  |
| 6 | **Disc Filter filter surface 1200qcm, max pressure 10 bar, max flow 30 (m3/h), 120Mesh, 2"BSP Male Thread, (made in China or Turkey)** | **Each** | **1.00** |  |  |
| 7 | **End Line, Dn16, (made in China or Turkey)** | **Each** | **100.00** |  |  |
| 8 | **Safety Ring, Dn16, (made in China or Turkey)** | **Each** | **200.00** |  |  |
| 9 | **Straight Connector, Dn16, (made in China or Turkey)** | **Each** | **50.00** |  |  |
| 10 | **Stainless Steel Pressure Gauge (L), 3" display, (made in China or Turkey)** | **Each** | **2.00** |  |  |
| 11 | **Fittings set** | **lump-sum** | **1.00** |  |  |
| 12 | **5 HP submersible water pump, capacity 10m3/h (JD, Dongyin, Vackson) along with the required 100m power cable** | **Each** | **1.00** |  |  |
| 13 | **Delivery to Zabul Cricket Ground** | **lump-sum** | **1.00** |  |  |
| 14 | **Excavation of 1200m (30cm deep x 30cm wide) for burying the main pipe** | **Each** | **750.00** |  |  |
| 15 | **Survey, design and Installation** | **lump-sum** | **1.00** |  |  |
| **Sub Total/AFN** | | | | |  |
|  | | | | | |
| **NO** | **Description** | **Unit** | **Quantity** | **Unit Cost** | **Total Cost** |
| **Kunduz Cricket ground Drip irrigation System BOQ** | | | | | |
| 1 | **Turbulent Flowing On-line Dripper, 4L/h, Black Color (made in China or Turkey)** | **Each** | **2,000.00** |  |  |
| 2 | **Offtake for PVC Pipe, Dn,16, With T type Grommet (made in China or Turkey)** | **Each** | **100.00** |  |  |
| 3 | **LLDPE Lateral pipe, outside Dia 16mm, 1.2mm thickness, 4.0bar, Laser print Φ16\*1.2 500m 1m/laser, One Bule Line on pipe** | **Meter** | **1,500.00** |  |  |
| 4 | **HDPE Pipe 1.5" (50mm) SDR 17, PN 10, PE 100 quality (50 years warranty)** | **Meter** | **500.00** |  |  |
| 5 | **HDPE Pipe 1.25" (40mm) SDR 17, PN 10, PE 100 quality (50 years warranty)** | **Meter** | **250.00** |  |  |
| 6 | **Disc Filter filter surface 1200qcm, max pressure 10 bar, max flow 30 (m3/h), 120Mesh, 2"BSP Male Thread, (made in China or Turkey)** | **Each** | **1.00** |  |  |
| 7 | **End Line, Dn16, (made in China or Turkey)** | **Each** | **100.00** |  |  |
| 8 | **Safety Ring, Dn16, (made in China or Turkey)** | **Each** | **200.00** |  |  |
| 9 | **Straight Connector, Dn16, (made in China or Turkey)** | **Each** | **50.00** |  |  |
| 10 | **Stainless Steel Pressure Gauge (L), 3" display, (made in China or Turkey)** | **Each** | **2.00** |  |  |
| 11 | **Fittings set** | **lump-sum** | **1.00** |  |  |
| 12 | **5 HP submersible water pump, capacity 10m3/h (JD, Dongyin, Vackson) along with the required 100m power cable** | **Each** | **1.00** |  |  |
| 13 | **Delivery to Zabul Cricket Ground** | **lump-sum** | **1.00** |  |  |
| 14 | **Excavation of 1200m (30cm deep x 30cm wide) for burying the main pipe** | **Each** | **750.00** |  |  |
| 15 | **Survey, design and Installation** | **lump-sum** | **1.00** |  |  |
| **Sub Total/AFN** | | | | |  |
| **Grand Total/AFN** | | | | |  |
|  | | | | | |

* ***Goods warranty \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_months after installation and completion of the works.***
* ***Technical training to ACB staff free of cost till six months Yes/No***
* ***Project completion period after signing the contract\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ days***
* ***Transportation and accommodation charges during 6 month is the supplier responsibility.***

**Documentation Required with the Submission of the Quotation**

The Supplier shall attach the following documents to its quotation’s

* + A duly completed and signed priced offer as per the Schedule of Items and the Priced Quotation. Note that all prices shall be quoted in AFN;
  + a valid Trade License
  + a valid Business Bank Account.
  + Must have Similar experience document (one or two contracts).

The winner company may compulsorily provide the above requirement.

**Correction of Errors**

Quotations determined to be substantially responsive shall be checked by the Purchaser for any arithmetic errors. Errors shall be corrected by the Purchaser as follows:

* where there is a discrepancy between the amounts in figures and in words, the amount in words shall govern; and
* where there is a discrepancy between the unit rate and the line-item total resulting from multiplying the unit rate by the quantity, the unit rate as quoted shall govern, unless in the opinion of the Purchaser there is an obviously gross misplacement of the decimal point in the unit rate, in which case the line-item total as quoted shall govern, and the unit rate shall be corrected.

The amount stated in the Quotation shall be adjusted by the Purchaser in accordance with the above procedure for the correction of errors and, with the concurrence of the Bidder, shall be considered as binding upon the Bidder.

**Payments:**

The following payment terms shall be applied for the contract:

* All payments shall be subjected to Afghanistan income tax law.
* Payment will be made to selected vendor through bank account or cheque.
* International Business Bank Account if have.
* Payment through Business Bank account (National) will be made in 15 working days after delivery and completion of the works.